**Market research "Restoring and ensuring the operation of the LCD monitors**

**of the passenger information system in the vehicles of RM LLC Rīgas satiksme”**

Answers to the questions submitted by the Applicant (07.08.2024.):

|  |  |  |
| --- | --- | --- |
| **Technical specification point** | **Applicant's question** | **Customer's response** |
|  | LCD monitor dimensions and required image parameters - need to specify what does it mean *3x10,5“*” (for trams). Is ir *10,5 inch = 266,7 , width is around 20 cm , 20 cm x 3 display = 60 cm* | The tram (model 15T, 15T1) has 3 LCD monitors on-board, the size of each monitor is 10,5 inches. |
|  | LCD display resolution? | 1920 x 1080 |
|  | Certification requirements:  Bus  Tram | According to the technical documentation of the vehicle which is available on site upon arriving in person at the Customer's office, according to the confidentiality agreement with the vehicle suppliers.  Please coordinate the time of arrival in advance with the Customer's contact person specified in the Application. |
|  | Serial ports? |
|  | Software interface description:  how displays interface with router/back-end software? |
|  | Display control description (GNSS data, other control data) |